Haulotte 4527 A Articulated & telescopic trailer

[Technical data](http://www.haulotte-usa.com/product/4527%22%20%5Cl%20%22collapseOne)

|  |  |
| --- | --- |
| Working height | 51 ft |
| Platform height | 45 ft |
| Horizontal outreach (from centerline) | 27 ft |
| Horizontal outreach (from edge of footpad) | 21 ft |
| Up and over height | 20 ft 9 in |
| Lift capacity | 500 lbs |
| Length - stowed | 20 ft 8 in |
| Width stowed | 5 ft 6 in |
| Height stowed | 6 ft 8 in |
| Platform size | 4 ft 1 in x 2 ft 9 in |
| Turntable rotation | 350° non-continuous |
| Jib - length | 4 ft 3 in |
| Jib - Vertical Motion | 150° (+70 / -80) |
| Tow speed rating | 65 mph |
| Leveling capability | 12.5 ° |
| Tire size | ST 225/75 R15 |
| Power source | 4 x 6 V 245 amp-hr |
| Tongue weight (no options) | 290 lbs |
| Weight (no options) | 4200 lbs |
| Widest Point | 13 ft 9 in |
| Widest Point | 13 ft 6 in |